More info here:

http://www.40percent.club/2018/02/fourty_two.html

[How to order PCBs from gerber files](http://www.40percent.club/2017/03/ordering-pcb.html)

EasyEDA ordering info:

PCB

![42front](42front.png)
![42back](42back.png)

Gerber: fourtytwo.zip

    204.8mm Max* 71.4mm Max;
    Layers: 2;
    PCB Thickness: 1.6mm;
    PCB Qty.: 10;
    PCB Color: Green;
    Surface Finish: HASL;
    Copper Weight: 1;
    Panelized PCBs: 1


![42top](42top.png)

Gerber: fourtytwo top.zip

    214.3mm Max* 81.0mm Max;
    Layers: 2;
    PCB Thickness: 1.6mm;
    PCB Qty.: 5;
    PCB Color: Green;
    Surface Finish: HASL;
    Copper Weight: 1;
    Panelized PCBs: 1


![42bottom](42bottom.png)

Gerber: fourtytwo bottom.zip

    214.3mm Max* 81.0mm Max;
    Layers: 2;
    PCB Thickness: 1.6mm;
    PCB Qty.: 5;
    PCB Color: Green;
    Surface Finish: HASL;
    Copper Weight: 1;
    Panelized PCBs: 1


Files released under https://creativecommons.org/licenses/by-nc-sa/4.0/

![Creative Commons Attribution-NonCommercial-ShareAlike 4.0 International License](https://i.creativecommons.org/l/by-nc-sa/4.0/88x31.png)
